BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1914
Charging method

T-interface:

The command is used to define the subscribed charging method for the current ISDN-link. It states whether charging is subscribed from the network operator and also the current subscribed charging method.

The following charging methods are available in BTUB and BTUDP:

- AOC charging not subscribed.
- AOC-D charging requested for each call setup to the network. Charging from network is done continuously during the call.
- AOC-E charging requested for each call setup to network. Charging from network is done at the end of the call.
- AOC-D charging from network is permanent. Charging from network is done continuously during the call.
- AOC-E charging from network is permanent. Charging from network is done at the end of the call.

Country specific settings

Country | AOC n.s | AOC D. | AOC E. | AOC perm
Australia | X | - | - | X
Austria | X | X | X | X
Belgium | X | - | - | X
Italy | X | - | - | X
Nether-lands | X | - | - | X
Sweden | - | - | - | -
Spain | - | - | - | -
Finland | X | X | X | X
Denmark | X | - | - | -
New Zealand | X | - | - | -

Q_interface:

The command defines the charging method for the current link which is requested from the originating PBX in the private network.

The following charging methods are available on BTUB and BTUDP:

- AOC charging not requested.
- Interim charging requested for each call setup to the private network. If interim charging is provided for the current call (positive request-answer from the public gateway exchange ) then charging information is received continuously during the call from private network.
- Final charging requested for each call setup to the private network. If final charging is provided for the current call (positive request-answer from the public gateway exchange) then charging information is received at the end of call from private network.

Note

INTERIM charging should be requested (programmed) in the originating exchange because the received AOC-information from private network is only used for display purposes yet (the extension’s display is updated only during call).

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003