BusinessPhone Communication Platform 4.0
Commands > Commands 9000...9999

## 9131
NPI for private/public called number 3

The command is used to define the Number Plan Identifier (Number Plan and Type Of Number) of the called number.

Following combinations of NP's and TON's are available for the CN calls:

NP | TON | Value
E.164 (ISDN) | International | PUB/INT
National | PUB/NAT
Subscriber | PUB/SUBS
Unknown | PUB/UNK
PRIVATE NP (QSIG) | Regional level 1 | PNP/RL1 (regional)
Regional level 0 | PNP/RL0 (local)
Unknown | PNP/UNK
UNKNOWN NP (QSIG) | Unknown | UNK/UNK

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003