BusinessPhone Communication Platform 4.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 16 E2RECRD

0EDh E2RECRDFST |  | Read first record linked to basic E2-record |
0EEh E2RECRDNXT |  | Read next record linked to basic E2-record |
0EFh E2BASPRMRD |  | Read programming model number of E2-base |
0F0h E2BASPRMWR |  | Write programming model number of E2-base |
0F1h E2RECPRMRD |  | Read programming model number of E2-record |
0F2h E2RECPRMWR |  | Write programming model number of E2-record |
01h CERECCREATE |  | Indication for application blocks that CE has seized additional E2 record (contents only data converted by CE) |

Revision: PD2 © Ericsson Enterprise 2003