BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0169
Directory number subscribed in PSTN ?

This command defines if the internal programmed directory number of the extension is in the subscribed PSTN number range. If the directory number is not in the number range, a common number defined by command 1801, is used in case of A- or B- number sending.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003