BusinessPhone Communication Platform 4.0
Commands > Commands 5000...5999

## 5405
Create Call Pickup Code

In ASB 150 a call pickup group is formed from a list of extensions. In case of a call to a member of the group another member can answer the call from his/her own telephone by dialling the code for “group call pickup”.

The actual facility can be created via this command. The facility is created by stating the directory number to be used for answer from any group member. The directory number must be free and must not conflict with existing directory numbers, see command group 56.

Command 5406 Create call pickup ext. group creates groups for this facility. Command 4201 State members in group defines which extensions are to be members of the group.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003