BusinessPhone Communication Platform 4.0
Dialogs

## Connection Parameters

To connect to the system, you must define the connection parameters first. The connection parameters are stored in the database and will be used by the system until you change them again.

To access the Connection Parameters dialog, open context menu of your system by clicking on the system’s name in the Configuration directory tree, and then select “Settings”.

After creating a new system, the default parameters are stored in the database. You can change them anytime by selecting the “Settings” option in the context menu of the system.

### Changing the connection parameters

To change the connection parameters of a system:

- Select a system from the Configuration directory tree or open a new system using the System Selection.
- Select “Settings” in the context menu.

The current connection parameters for the selected system are displayed.

In BMS there are five possible types of connection:

- Direct Serial – A system is connected directly to one of the COM ports of the computer on which the BMS Server is running.
- Direct Modem – BMS connects to the system, using a local modem.
- Remote serial – A system is connected directly to one of the COM ports of a computer on which a BMS Agent is running. BMS connects indirectly to the system using TCP/IP to the BMS Agent and then direct serial connection from the BMS Agent to the system.
- Remote modem – BMS connects indirectly to the system, using a TCP/IP connection to the BMS Agent and then by modem connection from the BMS Agent to the system.
- IPU (TCP)

Each connection mode has its own set of parameters. When you select a connection type in the list box, the corresponding set of parameters is displayed and can be edited.

#### Actions

Submit |  | To save the current parameters setting to the database. |
Default |  | To reset the parameter setting and to use the standard values for the respective parameter. |

### Parameters for direct serial connection

Connection Type | Selection box | Direct Serial
Required Access: | Selection box | Full, Read Only
Password | Edit field | *****
COM Port name | Edit field | COM1, COM2, …
Baud Rate | Selection box | 300, 600, 1200, 2400, 4800, 9600*, 7200, 12000, 14400, 19200
Data Bits | Selection box | 5, 6, 7, 8*
Stop Bits | Selection box | 1*, 2
Parity | Selection box | None*, Even, Odd
Flow Control In | Selection box | None*, Xon/Xoff, RTS/CTS
Flow Control Out | Selection box | None*, Xon/Xoff, RTS/CTS
Dect Connection Type | Selection box | No DECT system, Connection switching (only one connection to BusinessPhone; no cable to IC-CU2), Dual connection (2 connections to BusinessPhone; one separate cable to IC-CU2)
Distributor Password | Edit Field | Password with 5 digits
Keep up connection until last user | Selection box | logs out*, disconnects

### Parameters for direct modem connection

Connection Type | Selection box | Direct Modem
Required Access: | Selection box | Full, Read Only
Modem Connection Type | Selection box | Normal, Manual, Transfer, Callback
Password | Edit field | *****
COM Port name | Edit field | COM1, COM2, …
Baud Rate | Selection box | 300, 600, 1200, 2400, 4800, 9600*, 7200, 12000, 14400, 19200
Data Bits | Selection box | 5, 6, 7, 8*
Stop Bits | Selection box | 1*, 2
Parity | Selection box | None*, Even, Odd
Flow Control In | Selection box | None*, Xon/Xoff, RTS/CTS
Flow Control Out | Selection box | None*, Xon/Xoff, RTS/CTS
Dial Type | Selection box | Tone*, Pulse
Init String | Edit field | Enter init string for modem connection
Number | Edit field |
Dect Connection Type | Selection box | No DECT system, Connection switching (only one connection to BusinessPhone; no cable to IC-CU2), Dual connection (2 connections to BusinessPhone; one separate cable to IC-CU2)
Distributor Password | Edit Field | Password with 5 digits
Keep up connection until last user | Selection box | logs out*, disconnects

### Parameters for remote serial connection

Connection Type | Selection box | Remote Serial
Required Access: | Selection box | Full, Read Only
Agent Host | Edit field | Name or IP address
Agent Port | Edit field | 7777*
Password | Edit field | *****
COM Port name | Edit field | COM1, COM2, …
Baud Rate | Selection box | 300, 600, 1200, 2400, 4800, 9600*, 7200, 12000, 14400, 19200
Data Bits | Selection box | 5, 6, 7, 8*
Stop Bits | Selection box | 1*, 2
Parity | Selection box | None*, Even, Odd
Flow Control In | Selection box | None*, Xon/Xoff, RTS/CTS
Flow Control Out | Selection box | None*, Xon/Xoff, RTS/CTS
Dect Connection Type | Selection box | No DECT system, Connection switching (only one connection to BusinessPhone; no cable to IC-CU2), Dual connection (2 connections to BusinessPhone; one separate cable to IC-CU2)
Distributor Password | Edit Field | Password with 5 digits
Keep up connection until last user | Selection box | logs out*, disconnects

### Parameters for remote modem connection

Connection Type | Selection box | Remote Modem
Required Access: | Selection box | Full, Read Only
Modem Connection Type | Selection box | Normal, Manual, Transfer, Callback
Agent Host | Edit field | local host*
Agent Port | Edit field | 7777*
Password | Edit field | xxxxx
Port name | Edit field | COM1, COM2, …
Baud Rate | Selection box | 300, 600, 1200, 2400, 4800, 9600*, 7200, 12000, 14400, 19200
Data Bits | Selection box | 5, 6, 7, 8*
Stop Bits | Selection box | 1*, 2
Parity | Selection box | None*, Even, Odd
Flow Control In | Selection box | None*, Xon/Xoff, RTS/CTS
Flow Control Out | Selection box | None*, Xon/Xoff, RTS/CTS
Dial Type | Selection box | Tone*, Pulse
Init String | Edit field | Enter init string for modem connection
Number | Edit field |
Dect Connection Type | Selection box | No DECT system, Connection switching (only one connection to BusinessPhone; no cable to IC-CU2), Dual connection (2 connections to BusinessPhone; one separate cable to IC-CU2)
Distributor Password | Edit Field | Password with 5 digits
Keep up connection until last user | Selection box | logs out*, disconnects

### Parameters for IPU (TCP) connection

Connection Type | Selection box | IPU (TCP)
Required Access: | Selection box | Full, Read Only
Password | Edit field | *****
IPU IP Address | Edit field | 127.0.0.1*
IPU Port | Edit field | 6000*
Dect Connection Type | Selection box | No DECT system, Connection switching (only one connection to BusinessPhone; no cable to IC-CU2), Dual connection (2 connections to BusinessPhone; one separate cable to IC-CU2)
Distributor Password | Edit Field | Password with 5 digits
Keep up connection until last user | Selection box | logs out*, disconnects

### Personal Settings

Alternatively, you can use your personal settings. The personal settings can be entered, modified, activated or deactivated in the System Selection dialog.

To access the dialog, check the Use Personal Settings in the System Selection.

You can define the following personal settings:

- Agent Host - Name or IP address of the agent
- Agent port - Default is 7777
- Port Name - COMM port, default is COM1
- Dial Type - Tone or pulse for the modem dialling, default is Tone
- Init String- Modem initialization string
- Number Prefix - Modem number prefix
- If you want to use the password saved in the database, check “Use password from DB”.

The personal settings can be activated or deactivated. The System Selection dialog shows the status of your personal settings (“YES” or “NO”).

After modifying the personal settings, you can return to the Select system dialog by pressing the Back button in the control bar.

#### Actions

Submit |  | To submit your personal settings to the system. |
Default |  | To reset the dialog to default values. |
Back |  | To return to the System Selection dialog. |

Revision: A © Ericsson Enterprise 2003