BusinessPhone Communication Platform 4.0
Commands > Commands 3000...3999

## 3801
ACD-group number

Via this command it is possible to read the group affiliation of an ACD-group created.

Range of values = 0-7

The command does not allow writing. When a new ACD-group number is created by command 5407 Create ACD group, this is not always automatically the lowest free serial number. If there are no previously programmed ACD-group numbers, the first automatic serial number is to be programmed 0, the second 1 and so on.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003