BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0x52
Invalid BTU Category

Default definition: |  | ALARM + EXTERN + ACTIVE |
Used by block: |  | TR |
Category: |  | MAINTENANCE |

The given BTU category is not yet prepared. This warning indicates a programming error.

- D1: Card position
- D2: Individual number of BTU
- D3: Category

- 01h ... CFPR invoke rejected from network.
- 02h ... CFPR feature failure, AOC failed.
- FFh ... Undefined category.

- D4: Reason

- If D3 = 01h

- 02h ... Service not available
- 05h ... Supplemental service, interaction not allowed.
- FFh ... CFPR, unspecified reason.

- If D3 = 02h

- 01h ... Storage capacity exceeded.
- 02h ... Record save failed.
- 03h ... Record overwritten.
- 04h ... Record load failed.
- 05h ... Record unlink failed.

- If D3 = FFh

- FFh ... Undefined reason.

#### Recommended action

Check the programming of the external lines.

Revision: F © Ericsson Enterprise 2003