BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0xBF
Wakeup Error

Default definition: |  | ALARM + INFO + EXTERN + ACTIVE |
Used by block: |  | HO |
Category: |  | DESIGNER |

The warning is sent, if, after a wakeup call has been rerouted to the front desk, the front desk cannot be contacted due to some error condition.

- D1: Directory number of extension, where wakeup failed, high byte
- D2: Directory number of extension, where wakeup failed, low byte
- D3: Undefined
- D4: Undefined

Revision: F © Ericsson Enterprise 2003