BusinessPhone Communication Platform 4.0
Dialogs

## Hardware survey – Card Selection

In this OFFLINE - dialog, you can select the type of card that is located in a cabinet’s board position shown on top of the dialog.

To access the dialog, click on the “Boards” menu in the Configuration directory tree. The context menu appears. Select “Hardware survey” from the context menu to open the Hardware survey dialog. Now click on one of the “...” buttons behind a cabinet position to open the Card Selection dialog.

For more information, see section Hardware survey and Installation Instruction ASB 150 02 (1531-ASB 150 02 Uen).

### Card Types

The following card types are available:

- CPU

- CPU D, CPU D-

- ELU

- ELUD 8; ELUD 16; ELUD 32; ELUA 8; ELUA 16; ELUC 10

- ICCU

- ICCU 8; ICCU 16; ICCU 24; ICCU 32; ICCU 48; ICCU 64; ICCU108; ICCU210

- BTU

- BTUA 4; BTUA 8; BTUB 8; BTUB 16; BTUD C; BTUD P

- IPU

- IPU 0; IPU 4; IPU 8; IPU 16

- Others

- MFU; MFU 2; VMU 16; VMUH 8; VMUH 16; AUX 1; AUX 2; REG 12.

Note

Non-self reporting cards are not available in this OFFLINE - dialog; non-self reporting cards can be added ONLINE only; see Hardware survey

### Selecting a card type

If you have selected a vacant position in the Hardware survey dialog, the radio button “empty” is marked. If you want to change an existing board position, the respective board type radio button is selected automatically.

Note

You cannot change the cabinet and board position in this dialog. To move boards go to Swap boards.

- Select a card type by clicking in the respective radio button.
- Click on Set to submit the changes.

- Or:

- Click on Close to abort the process and to return to the previous dialog without any changes.

#### Actions

Set |  | To set a board on the selected position. |
Next |  | To step to the next board position |
Previous |  | To step to the previous board position |
Close |  | To close the dialog and to return to the to the Hardware survey dialog. |

Revision: A © Ericsson Enterprise 2003