BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1302
Outgoing digit transmission

The command states how the digits are sent from the interworking exchange. The initial value depends on the type of the BTU.

Type of BTU: |  | Value: |
BTU-A |  | 0 |
BTU-C |  | 0 |
BTU-E |  | 0 |
BTU-D |  | 2 |

0 = |  | Decadic impulsing

1 = |  | DTMF

2 = |  | MFC

3 = |  | No sending of digits

4 = |  | MFE1 ( 2/5 )

5 = |  | MFE2 ( 2/6 )

Value = 0-5

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003