BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1009
Reroute on answering position barred ?

The command is to be used for in-dialing and for private lines to reroute calls to the rerouting position. Rerouting takes place if the call is made to a barred extension.

For rerouting to take place, the rerouting position must have been programmed, see commands 1103 Reroute position at day and 1104 Reroute position at night.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003