BusinessPhone Communication Platform 4.0
Commands > Commands 3000...3999

## 3082
Bypass Call diversion

This command specifies which ACOS (A-categories) are allowed to bypass call diversion and follow me.

Valid A-COS values: 0-15

Default value: N = ACOS is NOT allowed to bypass call diversion and follow me.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003