BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0xE8
FUNCTION ABORTED

Default definition: |  | ERROR |
Used by block: |  | MU |
Category: |  | MAINTENANCE |

A specific feature within ASB 150 02 was aborted. The associated functionality can be evaluated using the signal input, which cause the warning.

The definition of the warning code depends on the warning situation.

This warning code is open to be used by other software blocks as applicable.

- D1: -
- D2: Current state
- D3: INFCODE of the last received message
- D4: SUBCODE of the last received message

Revision: PD2 © Ericsson Enterprise 2003