BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1952
Signaling protocol

This command states the current ISDN-protocol to be used on the interface. It is possible to store various market-dependent ISDN protocols. The parameter defines selection of the current protocol to be used.

DMinimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003