BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0172
Fixed diversion destination for internal calls, if cordless is not available

This command is used to activate diversion on not available for internal calls. Diversion on not available could be a result of a not attainable cordless.

If no diversion address is specified, the diversion is inactive.

Note

After a call diversion “on not available”, no repeated call diversion is possible any more.

Valid data: 1 - 8 digit directory number

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003