BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1980
Packet Mode Communication Link parameters

This command is used to set-up and remove Packet Mode Communication links.

The maximum number of PMC links per board is 32 for BTU-B and 16 for MFU (BTUB) or a subequipped BTU-B. Up to three boards can be initiated with PMC links.

To set-up a PMC link between two ISDN interfaces (S/T) the parameters must be programmed properly:

- PMC link number, value = 1-32
- A-side interface number, value = 0-(6)14
- TEI value for the A-side, value = 0-63
- B-side interface number, value = 0-(6)14
- TEI value for the B-side, value = 0-63

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003