BusinessPhone Communication Platform 4.0
Commands > Commands 6000...6999

## 6703
Printout Header 1

This command can be used to define Line 1 of the printout header of call metering data. Here you can define a text of 50 characters for the first line of the header information.

6703 |  | Printout header 1

6704 |  | Printout header 2

6705 |  | Printout header 3

6706 |  | Printout header 4

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003