BusinessPhone Communication Platform 4.0
Commands > Commands 5000...5999

## 5605
Trunk directory number

Using this command it is possible to allot the required number to a trunk’s line position (ppiii).

If this line position already has a directory number it will be overwritten. Command 5902 Line position-directory number will read the directory number for a certain line position. However, references to previous numbers will remain. These references are to be deleted or replaced. See the description of command group 56 listing the commands referring to directory numbers.

If no number is indicated, any previous directory numbers for this line position are deleted and the line position no longer has a number. The previous number is now vacant, and a call towards this number will receive the vacant tone supplied by the exchange. However, incoming calls on this trunk will be routed to the trunk’s answering position.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003