BusinessPhone Communication Platform 4.0
Commands > Commands 9000...9999

## 9145
Complete called party NL 4

91 x 5 Complete called party number length (C-NL) This command states the total amount of digits in called party number which is required before a CN call setup/seizure is started to the network. The digit dialling is supervised with register timer in accordance to command 1403 Time supervision of short register sign. alt. MFC/MFE outgoing. If the timer elapses then the call-setup is started without any further number length control.

Value = 1-32

not programmed = blank (ordinary called number handling)

This C-NL category for private network router overrides the C-NL trunk category (command 1317 Complete called party number length). For proprietary CN calls the complete called party number can be separated into a ‘Subscriber number part’ and a ‘Dialled number part’: The length of the Subscriber number part (S-NL) can be defined in command 91 x 6 and is used to identify the called subscriber, i.e to reach a CN PBX. This number part is the most significant number part of a complete number. The ‘Dialled number part’ will be the least significant number part of a complete number. This number part will be transferred as proprietary information via UUS 1 and it is used for continued addressing within the reached CN PBX.

e.g.: At CN VPN call a private network number is translated to corresponding public number and thereafter separated as:

C-NL = |  | 13 |  | 0222 81100 |  | 4701 |  | (Complete called party number) |
S-NL = |  | 9 |  | 0222 81100 |  |  |  | (Subscriber number part) |
|  |  |  |  |  | 4701 |  | (Dialled number part) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003