BusinessPhone Communication Platform 4.0
Commands > Commands 9000...9999

## 9112
Remove digits choice 1

The network location access code can be modified due to selected route/destination. 1 up to 4 digits can be removed from the network location access code. The network location access code (modified or not) is transmitted before the predigits (command 9113 Predigits choice 1) and dialled external number.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003