BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1911
Network signalling protocol

The command is used to define the network signalling protocol for the current ISDN-link.

Available network signalling tables for T-reference point, DSS1, are:

- Australia
- ETSI
- Belgium
- Italy
- Netherlands
- Sweden
- Spain
- Finland
- Denmark
- New Zealand
- Swissnet
- Bezeq
- Network 2
- Network 3

Available network signaling tables for Q-reference point, QSIG, are:

- ETSI/ECMA + ETSI/ISO

Used initial values: DSS1.... ETSI network signalling QSIG.... ETSI/ECMA network signalling

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003