BusinessPhone Communication Platform 4.0
Commands > Commands 3000...3999

## 3803
Time for 2nd recorded answer

Recorded announcements can be supplied for calls to an ACD-group. Two recorded announcements can be programmed for ACD. This command is used to state the time to elapse before the 2nd recorded announcement is sent.

Value = 0-255 s

If the time is set to 0, no recorded announcement will be sent.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003