BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0x33
Invalid Message Length In Message

Default definition: |  | ERROR + TRIG |
Used by block: |  | ALL |
Category: |  | DESIGNER |

The length of the received message is not valid. This code is intended for programs, that use the ML byte to evaluate the data in the message. A message length, that is otherwise outside the valid range, is detected by OS.

- D1: Received message length (ML)
- D2: Received INFCODE
- D3: Received SUBCODE
- D4: Received DATA+1

If ‘OS.WARNING code,DY’ is not used, data D3 and D4 are supplied by OS from the ME-register.

Revision: F © Ericsson Enterprise 2003