BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2034
Initiate dial tone at LCR

This command defines whether or not a dial tone should be transmitted to the caller after dialling the directory number of a trunk which is controlled by LCR.

Y .... |  | Initiate dial tone sending

N .... |  | Do not initiate dial tone sending

See: |  | Command 1026 LCR analysis required

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003