BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0159
Direct diversion at internal
calls ?

The command defines whether or not a direct diversion on an internal call should be done.

If the extension is a master and a member of a tandem configuration the command data shall be copied to the slave and blocked for the slave's further use.

Default value: NO

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003