BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1921
Ignore inband info at disconnection

This command states whether inband information, which is available after DISCONNECT message, shall be ignored and immediate call clearing shall be initiated, or if the inband information (e.g. disconnection tone) shall be transmitted to the user.

Valid data:

NO = Inband information is not ignored (the user receives the inband information). |  |

YES = Inband information is ignored (the call is immediately released). |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003