BusinessPhone Communication Platform 4.0
Commands > Commands 4000...4999

## 4104
Receiving of tone signals

The command defines if the operator should receive tone signals during traffic indicating several cases in addition to the indication on the display.

Alternatives:

NO: |  | Additional tone signals are disabled. The operator will receive the display information for several traffic cases.

YES: |  | The operator will receive tone signals.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003