BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2003
National key (Inquiry)

Text to be printed on a printer or shown on a display can be defined via DIALOG 2753, DIALOG 2754, DIALOG 2662 and DIALOG 2663.

The following survey shows both non-programmable and programmable keys. The table shows only the keys for system instruments. The corresponding keys on operator instruments have the same values.

KEY | DIALOG 2662 | DIALOG 2753
ASCII | Character | ASCII | Character
0-9 | 30-39 | 0-9 | 30-39 | 0-9
* | 2A | * | 2A | *
# | 23 | # | 23 | #
A-Z | 41-5A | A-Z | 41-5A | A-Z
INQUIRY | **) | (Command 2003) | **) | (Command 2006)
HOLD | **) | (Command 2004) | 2E | .
READ & | **) | (Command 2005) | 20 | Space
TRANSFER | **) | (Command 2006) | 3A | :
SAVE | 20 | Space | 27 | ‘
CONF | 2E | . | -- |
LINE 1 | 2F | / | **) | (Command 2004)
LINE 2 | 27 | ‘ | **) | (Command 2005)
DIVERSION | 3F | ? | **) | (Command 2003)
MUTE | -- |  | 2D | -
PICKUP | -- |  | 2F | /
MENU *) | 2B | + | 2B | +
INFO *) | 2D | + | 2C | ,
MESSAGE *) | 2D | & | 26 | &
PROG *) | -- |  | 3D | =
F1 *) | 21 | ! | 21 | !
F2 *) | 3A | : | 3F | ?
F3 *) | 2C | , | 28 | (
F4 *) | 26 | & | 29 | )

**) |  | By means of commands 2003 National key (Inquiry)-2006 National key (Transfer) it is possible to select the character to be shown on depression of a key.

*) |  | These keys cannot be used for input of text for all facilities.

The table below lists the characters that are obtained for different values of the data in the command.

ASCII | Function
20-7D | Standard US ASCII
D1-FF | Special characters

STANDARD US ASCII, 20-7D

| 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | A | B | C | D | E | F
20 |  | ! | “ | # | $ | %% | & | ‘ | ( | ) | * | + | , | - | . | /
30 | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | : | ; | < | = | > | ?
40 | @@ | A | B | C | D | E | F | G | H | I | J | K | L | M | N | O
50 | P | Q | R | S | T | U | V | W | X | Y | Z | [ | \ | ] | ^ | _
60 | ‘ | a | b | c | d | e | f | g | h | i | j | k | ] | m | n | o
70 | p | q | r | s | t | u | v | w | x | y | z | { | | | } | -> | <-

SPECIAL CHARACTERS, D1-FF

Values for which no character is given are not defined.

D1 = |  | †

D2 = |  |

D3 = |  | •

D4 = |  | š

D9 = |  | ›

DA = |  | ‘

DB = |  | Empty square

DC = |  | “

DF = |  | ø

E1 = |  | “

ED = |  | ¨

EE = |  | ¤

EF = |  | (tm)

F5 = |  |

FC = |  | ‘

FF = |  | þ

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003