BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2530
Diversion address for fictive numbers

This command is used to state diversion addresses, for fictive directory numbers, to which incomming calls to the fictive number are diverted to.

For this command the number is not checked. However diversion will be executed only if the number is one of the following:

- extension number
- PBX-operator number
- extension (PBX) group number
- voice message number
- fictive number
- standard paging number
- automated attendant number
- private network number

Common abbreviated numbers are not allowed to be used as diversion address in order to prevent misuse of the facility to establish external calls.

The diversion address is erased by overwritting the directory number with blanks.

For the diversion to take place it is only necessary to programm a diversion address.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003