BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1013
Dial tone to extension ?

The command is used to determine whether or not a dial tone shall be sent to callers (A-party) in case of outgoing calls.

(Command 1307 PTS-signal from parent exchange ? is used to indicate whether a proceed-to-send signal is sent by the exchange, and command 1308 PTS-signal from parent exchange = dial tone ? is used to indicate if the proceed-to-send signal is the dial tone.)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003