BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0xA1
Serial Communication Pollerror

Default definition: |  | ERROR |
Used by block: |  | SP |
Category: |  | MAINTENANCE |

A request to send has been received from a regional processor (the EIRQ line has been pulled low), but no transmit was done.

- D1:
- D2:
- D3: Undefined
- D4: Undefined

Revision: F © Ericsson Enterprise 2003