BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1956
MSN provided to TEs ?

This command states whether MSN (Multiple Subscriber Number) is provided by the terminal user(s) on the interface. If it is not provided,the called party number information is discarded and a global call is indicated to the interface.

Valid data:

No |  | MSN is not provided

Yes |  | MSN is provided

Note

This feature can only be used, if the ISDN-terminals are programmed also with the MSN number!

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003