BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0x6F
IO Error

Default definition: |  | ALARM + EXTERN + ACTIVE |
Used by block: |  | EU |
Category: |  | DESIGNER |

Some error has been detected in IO handling for V24 or MODEM port.

- D1: Type of error.

- 01h: I/O port locked after repeated errors.
- 02h: Message lost (IOMESS used by local or remote O&M)
- 03h: Message timeout (usage as above)
- 04h: Timer request failed for no apparent reason.
- 05h: Invalid Multichannel command received.

- D2: Card position
- D3: Undefined
- D4: Undefined

Revision: F © Ericsson Enterprise 2003