BusinessPhone Communication Platform 4.0
Commands > Commands 4000...4999

## 4101
Operator line position

This command is used to state the position of those extension positions to which an operator is to be connected.

The line position is entered as: ppiii

where

pp = |  | board position (00-63)

iii = |  | individual (000-107)

A maximum of three operators are permitted.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003