BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8798
Automated attendant

This command group consists of commands to define the parameters for the Automated Attendant. First one or more directory numbers for the Automated Attendant (see command 5424 Create automated attendant) must be created. By entering command group 8701 General-announcement reference an existing directory number must be entered. Now all parameters are related to this voice menu.

Command 8701: |  | Defines the general announcement of the menu. For the Automated Attendant exists a special announcement group (see command 4411 AA reference number) designed to contain voice prompts for 32 voice menus. |
Command 8702: |  | Defines the error announcement for the menu (see also command 4411 AA reference number). |
Commands 8703-8712: |  | Defines the corresponding directory number of the received digit. |
Command 8713: |  | Defines the rewriting position in case of response or resource errors. |
Command 8714: |  | Defines if the menu is waiting for one digit or a full directory number. If this command is set to YES, the programming of the commands 8701-8712 is irrelevant. |

Minimum required authority level from telephone:

Accessible via BMS:

Revision: A © Ericsson Enterprise 2003