BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8102
Number of display digits

The paging receiver can manage display messages that have 0-10 digits. Display messages are presented on the display of the paging receiver in order to supply information to the pagee relevant to the pager or origin of the call.

This command is used to determine how many digits may be sent in a display message. Range of values 1-10 digits.

If the display message contains fewer digits than stipulated, initial zeroes will be added in the case where no end character is to be sent the paging equipment. See also command 8107 End of paging number.

If the display message contains more digits than stipulated, the final digits will be sent with standard paging, whereas the extension receives congestion tone for alternative paging.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003