BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8106
Display string

This command is used to determine the display message shown on the display of the paging equipment for an external (transferred) call.

If no digits have been stated, the relevant answer number (call number for answer + B-number = meet-me answer) will be shown.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003