BusinessPhone Communication Platform 4.0
Commands > Commands 6000...6999

## 6701
I/O Port

This command can be used to define the board number and the individual number of the I/O port, where call metering data should be output.

Value:

bbiii |  |

bb: |  | the board number where the printer port is located

iii: |  | the individual number of the printer port on the board

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003