BusinessPhone Communication Platform 4.0
Commands > Commands 6000...6999

## 6104
12h mode, display

You may enter the time in 12- or 24-hour-mode. (Independent of this programming, entering the time at a telephone is always done in the 24-hour mode, e.g. at wake-up call, reminder, setting of time.)

Enter the relevant function:

Y = |  | 12-hour mode

N = |  | 24-hour mode

Minimum required authority level from telephone: 1

Accessible via BMS: No

Revision: A © Ericsson Enterprise 2003