BusinessPhone Communication Platform 5.1
Commands > Commands 9000...9999

## 9101
Destination PBX

The dialled private network access number will associated to ‘type of corporate network call’, parameter indicating if call setup destination is ‘proprietary PBX’ (BP.MD) or ‘other vendor PBX’.

If destination is ‘proprietary PBX’ the type of network call is ‘proprietary corporate network call’ or ‘other vendor PBX’ then type of network call is ‘non-proprietary corporate network call’.

This information is used to activate/deactivate proprietary services for the started call setup.

Valid data:

0 = ‘proprietary PBX’ |  |

1 = ‘other vendor PBX’ |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003