BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1023
Trunk line type

The command is used to state to which type of trunk the BTU is connected.

0 = Trunk to a public exchange (PE)

1 = Trunk from a public exchange with direct in-dialing (INDIALING)

2 = Trunk to a private exchange, tie line (TIE LINE)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003