BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4603
Record announcements allowed ?

It is possible to determine whether or not a certain VMU board may be used for voice announcements.

Default value: NO = Voice announcement can not be stored on board.

Valid Values: YES / NO

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003