BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1712
EOS-signal?

The command is used for outgoing traffic to state whether the EOS-signal shall be received after the interworking exchange has received the full number.

Note

Ascertain that the signal is included in the selected signal diagram.

Valid Values: YES / NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003