BusinessPhone Communication Platform 5.1
Commands > Commands 8000...8999

## 8107
End of paging number

This command is used to determine whether an end character is to be used or not.

For DTMF-signalling the end character (#) can be sent to the paging equipment. The end character informs the paging equipment that all digits have been sent.

If no end character is used, the maximum number of digits will be sent to the paging equipment. See also command 8102 Number of display digits.

Valid values: YES / NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003