BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3902
Second voice answer

This command states the reference numbers for the second voice answer. Two references per voice answer and ACD-call number can be specified.

The reference number is entered as: uuvv

uu = 01 (always) |  |

vv = 01-32 (VIEW command 4401 Voice Announcements) |  |

uuvv = 0000 (no voice answer) |  |

It is required that the stated reference (uuvv) has been recorded with a system telephone in accordance with command 4401 Voice Announcements.

To obtain the automatic “number” indication it is required that “hours” are programmed in accordance with command 4405 Hours.

If only one reference is specified, only a voice answer in accordance with the stated reference will be obtained. The automatic “number” indication will not be received.

See command 3803 Time for 2nd recorded answer for programming of the time for the second voice message.

This command requires that ACD-group numbers have been created via command 5407 Create ACD group.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD4 © Ericsson Enterprise 2003