BusinessPhone Communication Platform 5.1
Commands > Commands 6000...6999

## 6203
Block log output?

The command is used when a temporary stop of logged call data is desired. During temporary stops in output the logged call data will be stored internally in the PABX. Temporary stops in output can be desirable during maintenance of connected external/peripheral equipment, e.g. in order to insert paper in a printer.

It should be noted that only a limited number of call records can be stored internally in the PABX. If the PABX's internal storage capacity is exceeded, it may be decidee whether or not to block outgoing external calls from the PABX, see command 6304 Bar outgoing calls?.

Valid values: YES / NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2003