BusinessPhone Communication Platform 5.1
Dialogs

## Configuration/Initialization

If the DECT system has not been initialized yet, this dialog will appear before you can proceed. If available, the dialog shows the default values for your country.

The Configuration/Initialization dialog consists of the following parts:

- B-ARI (for init, read-only later on)
- Set password
- CPU settings
- Wait for dial tone (different from country to country)
- Ringing cadences (from BMS 2001)
- System Tests
- Carriers
- SPU-S parameters

To apply the change of some values, you must reset the system first. If you submit a value that needs a system reset for activation, an additional message box will appear and ask you to reset the system.

Revision: B © Ericsson Enterprise 2003