BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2342
Traffic check at call pick-up

This command states how the traffic group check should be executed for -

- individual call pickup
- group call pickup
- common call pickup

Alternatives:

0 = Always allowed, no traffic group control. |  |

1 = The traffic group has to be open in at least one direction between the parties. |  |

2 = The traffic group has to be open in both directions between the parties. |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003