BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2271
Number of Automatic Redial Requests

This command defines the number of automatic redial requests which are allowed in ASB150 02 at the same time.

The parameter is used to limit the system resources.

##### Valid data:

Valid values: |  | 20, 30, 40 |
Initial values (default): |  | 30 |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003